- NAME
- SYNOPSIS
- DESCRIPTION
- OPTIONS
- NOTES
- SEE ALSO
- COPYRIGHT

# NAME

dsaparam - DSA parameter manipulation and generation

# SYNOPSIS

gmssl dsaparam [-help] [-inform DER|PEM] [-outform DER|PEM] [-in filename] [-out filename] [-noout] [-text] [-C] [-rand file(s)] [-genkey] [-engine id] [numbits]

# DESCRIPTION

This command is used to manipulate or generate DSA parameter files.

# OPTIONS

-help

  Print out a usage message.

-inform DER|PEM

  This specifies the input format. The DER option uses an ASN1 DER encoded form compatible with RFC2459 (PKIX) DSS-Parms that is a SEQUENCE consisting of p, q and g respectively. The PEM form is the default format: it consists of the DER format base64 encoded with additional header and footer lines.

-outform DER|PEM

  This specifies the output format, the options have the same meaning as the -inform option.

-in filename

  This specifies the input filename to read parameters from or standard input if this option is not specified. If the numbits parameter is included then this option will be ignored.

-out filename

  This specifies the output filename parameters to. Standard output is used if this option is not present. The output filename should not be the same as the input filename.

-noout

  this option inhibits the output of the encoded version of the parameters.

-text

  this option prints out the DSA parameters in human readable form.

-C

  this option converts the parameters into C code. The parameters can then be loaded by calling the get_dsaXXX() function.

-genkey

  this option will generate a DSA either using the specified or generated parameters.

-rand file(s)

  a file or files containing random data used to seed the random number generator, or an EGD socket (see RAND_egd(3)). Multiple files can be specified separated by an OS-dependent character. The separator is ; for MS-Windows, , for OpenVMS, and : for all others.

numbits

  this option specifies that a parameter set should be generated of size numbits. It must be the last option. If this option is included then the input file (if any) is ignored.

-engine id

  specifying an engine (by its unique id string) will cause dsaparam to attempt to obtain a functional reference to the specified engine, thus initialising it if needed. The engine will then be set as the default for all available algorithms.

# NOTES

PEM format DSA parameters use the header and footer lines:

     -----BEGIN DSA PARAMETERS-----
     -----END DSA PARAMETERS-----

DSA parameter generation is a slow process and as a result the same set of DSA parameters is often used to generate several distinct keys.

# SEE ALSO

gendsa(1), dsa(1), genrsa(1), rsa(1)

# COPYRIGHT

Copyright 2000-2016 The OpenSSL Project Authors. All Rights Reserved.

Licensed under the GmSSL license (the "License"). You may not use this file except in compliance with the License. You can obtain a copy in the file LICENSE in the source distribution or at https://www.openssl.org/source/license.html.